M-Tech R418W2 486 Motherboard BIOS Images



Note: Trying to flash the BIOS directly on the M-Tech R418W2 motherboard may
result in checksum and memory errors. With this particular motherboard model
it has been found you have to remove the BIOS chip from the M-Tech R418W2
motherboard and place it into another motherboard (a Socket 8 model was used
in testing) so you can flash it properly. A method called “hot flashing”
will probably be required. If you are unfamiliar with hot flashing a BIOS then
please seek out someone that is familiar with this technique as you could brick
your chip. UniFlash v1.4 was used to backup and flash the BIOS images.



BIOS IMAGES IN CHRONOLOGICAL ORDER:

———————————————————————————————————


1.) R418F2.BIN (oldest)

2.) R418G.BIN

3.) R418H.BIN

4.) R418I.BIN

5.) R418KW.BIN (final & latest release)