
JUNE 2015

From alecv of the Vintage Computer Forums:

"This card is SB Pro-like and contains rudimental 'mixer'. By default (after reset) all channels are muted.
Card itself works, but produces silence. This 'driver' just enables 'mixer'.

The SCSI pard is standard TMC-950."